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	عنوان مدرك:  دستورالعمل اجرایی دستگاه  FT-IR

Title: FT-IR ATR  Bruker EquipmentWorking Instruction


	كدمدرك:
WI- RC- 013
	بازنگری:
----



	1- هدف: 
هدف از تدوین این دستورالعمل، تشریح روند اجرای کار با دستگاهFT-IR ATR  با نام تجاریBruker ساخت کشور آلمان می باشد. 
2- دامنه عملکرد: 
این دستور العمل در بخش های مختلف آزمایشگاه کاربرد دارد. 
3- مسئولیت :
مسئولیت اجرای این دستور العمل با کارشناسان آزمایشگاه مربوطه می باشد. 
4- روش کار:
1- از روشن بودن قسمت اصلی دستگاه مطمئن شوید.
2- بعد از روشن کردن لب تاپ دستگاه، بر روی برنامه OPUS کلیک کرده و جهت ورود پسورد "OPUS" را وارد کنید.
3- اجازه دهید تا نرم افزار برنامههای آماده سازی را به اتمام برساند.
4- به نسبت 1/20 از ماده مورد آنالیز/KBr را داخل هاون ریخته و کاملا پودر نمایید.
5- قبل از گرفتن طیف نمونه مورد نظر، مزاحمت محیطی را با اندازهگیری پس زمینه حذف کنید.
6- بعد از آماده سازی نمونه، به کمک نگاهدارنده دستگاه، قرص ساخته شده را داخل دستگاه گذاشته و سپس طیف نمونه قرص را بگیرید.
7- بعد از اتمام کار و خاموش کردن لب تاپ، دستگاه را در حالت روشن رها کنید.
در صورت نیاز به استفاده از ATR، با کارشناس آزمایشگاه به منظور آماده سازی دستگاه هماهنگ کنید.    








	1. Purpose: 
The purpose of this procedure is to describe the operating procedure for the FT-IR ATR instrument, Bruker brand, manufactured in Germany.
2. Scope: 
This procedure is applicable to the different sections of the laboratory.
3. Responsibility: 
The laboratory personnel responsible for the relevant section are responsible for implementing this procedure.
4. Procedure:
1. Ensure that the main unit of the instrument is switched on.
2. After switching on the instrument laptop, open the OPUS software and enter the OPUS password to log in.
3. Allow the software to complete its initialization and preparation procedures.
4. Mix the material to be analyzed with KBr at a ratio of 1:20 and thoroughly grind the mixture in a mortar until it is completely powdered.
5. Before acquiring the spectrum of the sample, eliminate environmental interference by measuring the background spectrum.
6. After preparing the sample, place the prepared pellet into the instrument using the sample holder, and then acquire the spectrum of the sample pellet.
7. After completing the analysis and shutting down the laptop, leave the instrument switched on.
If ATR measurement is required, coordinate with the laboratory technician responsible for preparing the instrument.
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