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	عنوان مدرك:  دستورالعمل اجرایی دستگاه آب خالص ساز 

Title: Milipore ultra pure waterEquipmentWorking Instruction


	كدمدرك:
WI- RC- 002
	بازنگری:
----



	1- هدف: 
هدف از تدوین این دستورالعمل، تشریح روند اجرای کار با دستگاهUltra-pure water  با نام تجاریMilipore  ساخت کشور آمریکا می باشد. 
2- دامنه عملکرد: 
این دستور العمل در بخش های مختلف آزمایشگاه کاربرد دارد. 
3- مسئولیت :
مسئولیت اجرای این دستور العمل با کارشناسان آزمایشگاه مربوطه می باشد. 
4- روش کار:
1- علامت + و – سمت راست دستگاه را همزمان فشار دهید.
2- اجازه دهید تا عدد18.2 MΩ.cm  بر روی صفحه نمایشگر دستگاه ظاهر شود.
3- کلید آبی روی دستگاه را فشار دهید.
4- بعد از برداشت آب مورد نظر با فشار دادن همان کلید خروجی آب را قطع کنید.
5- سپس محافظ زیر شیر را در سر جای خود قرار دهید.
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1. Purpose
The purpose of this procedure is to describe the operating procedure for the ultrapure water purification system, Millipore, manufactured in the USA.
2. Scope
This procedure is applicable to the various sections of the laboratory.
3. Responsibility
The responsibility for implementing this procedure rests with the relevant laboratory personnel.
4. Operating Procedure
1. Press the + and − buttons located on the right side of the instrument simultaneously.
2. Allow the display to show a resistivity value of 18.2 MΩ·cm.
3. Press the blue button on the instrument.
4. After collecting the required amount of water, press the same button to stop the water flow.
5. Return the protective cover below the dispensing outlet to its proper position.
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